**Comparison of purchasing costs of STUDS for the use in the SMS- kit**

Please try to get an offer of your local supplier for the below mentioned options:

**Qty: 10, 50, and 200 per option.**

**Option 1** *(as alternative for the US- market instead of option 3- SAMSON AG company standard)*

Continuous Thread Stud per B18.31.2

Size 3/4” – 10 UNC x 3 1/2,

Steel per ASTM A193 B7,

Zinc plated per ASTM F 1941 Fe/Zn-Ni 8A

**Option 2** *(US-version as comparison to option 3)*

Tap-End Studs per B18.31.2; full body, tap threaded end 1 1/8 x D, overall length 3 1/2

Size 3/4” – 10 UNC x 3 1/2,

Steel per ASTM A193 B7,

Zinc plated per ASTM F 1941 Fe/Zn-Ni 8A

**Option 3** *(current version – used for SMS NPS 3 CL600 WCC)*

Tap End Studs per Company Standard 2.21-65 sheet 6

**8324-8059** SPSL 1 – Material datasheet 1010-5397

3/4” -10 UNC -2A; length l =60 mm; length b1=28 mm

Zinc plated per ASTM F 1941 Fe/Zn-Ni 8A



