ITEM#1 @ 30 Each

BOLT HEX HEAD

SIZE HEAVY HEX 1/2 INCH -13UNC-2A X 2 INCH -1/2 LG,

QQ-N-286, K-MONEL, GRADE E-500, MIL-STD-1222, TYPE-II. MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#2@20 Each

BOLT HEX HEAD ,BOLT, MACHINE, HEAVY, HEX, K-500, SPECIFICATION K-MONEL, GRADE-500, QQ-N-286 CL-AMS-18116(H), MIL-DTL-1222(J) TYPE II, SIZE 1/2 INCH -13UNC-2A X 1-3/4 INCH LG.MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#3 @ 20 Each

STUD

K-MONEL, GRADE-500, QQ-N-286 CL-AMS-18116(H),

MIL-DTL-1222(J) TYPE IV, SIZE 5/8 INCH -11UNC-2A X 5 INCH LG. MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#4 @100 Each

BOLT HEX HEAD ,

BOLT, MACHINE, HEAVY, HEX, K-500, K-MONEL,

GRADE-500, QQ-N-286 CL-AMS-18116(H), MIL-DTL-1222(J) TYPE II, SIZE 5/8 INCH -11UNC-2A X 2-1/4 INCH LG.

MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#5@ 65 Each

BOLT HEX HEAD

BOLT, MACHINE, HEAVY, HEX, K-500, K-MONEL, GRADE-500, QQ-N-286 CL-AMS-18116(H), MIL-DTL-1222(J) TYPE II,

SIZE 5/8 INCH -11UNC-2A X 2-1/2 INCH LG.

ITEM#6@ 100 Each

BOLT HEX HEAD

BOLT, MACHINE, HEAVY, HEX, K-500, K-MONEL, GRADE-500, QQ-N-286 CL-AMS-18116(H), MIL-DTL-1222(J) TYPE II, SIZE 5/8 INCH -11UNC-2A X 3 INCH LG. MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#7@ 80 Each

BOLT HEX HEAD BOLT, MACHINE, HEAVY, HEX, K-500, K-MONEL, GRADE-500, QQ-N-286 CL-AMS-18116(H), MIL-DTL-1222(J) TYPE II,SIZE 5/8 INCH -11UNC-2A X 3-1/4 INCH LG. MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#8 @30 Each

BOLT HEX HEAD

HEX HEAD BOLT, SIZE 5/8 INCH -11UNC-2A X 2 INCH -1/4 LG, QQ-N-286, K-MONEL, GRADE E-500, MIL-STD-1222, TYPE-I. MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#9 @40 Each

BOLT HEX HEAD

SIZE 5/8 INCH -11UNC-2A X 2 INCH-1/2 LG, QQ-N-286, K-MONEL, GRADE E-500, MIL-STD-1222, TYPE-I. MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#10@ 40 Each

BOLT HEX HEAD

SIZE 5/8 INCH -11UNC-2A X 3 INCH LG, QQ-N-286, K-MONEL, GRADE E-500, MIL-STD-1222, TYPE-I. MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#11@ 40 Each

BOLT HEX HEAD

SIZE HEAVY HEX 3/4 INCH -10UNC-2A X 4 INCH -1/4 LG,

QQ-N-286, K-MONEL, GRADE E-500, MIL-STD-1222, TYPE-II. MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.

ITEM#12@ 40 Each

BOLT HEX HEAD

SIZE HEAVY HEX 3/4 INCH -10UNC-2A X 4 INCH -3/4 LG, QQ-N-286, K-MONEL, GRADE E-500, MIL-STD-1222, TYPE-II. MAGNETIC PERMEABILITY SHALL BE 2.0 OR LESS.