|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **No** | **Standard** | **Description** | **Type** | **Additional info** | **Coating** | **Qty** |
| **1** | GB32 1-88 | M20-2.5x65 Bolt | 8.8 Grade | Hex head with hole for wire locking | Dacro | 288 |
| **2** | GB/T 900-88 | M20-2.5x200 studs | 8.8 Grade | double ended bm=2d | Dacro | 24 |
| **3** | GB/T 900-88 | M20-2.5x240 studs | 8.8 Grade | double ended bm=2d | Dacro | 240 |
| **4** | GB889-86 | M20-2.5 Hex Nut | 8.8 Grade | Hex nut with lock | Galvanization | 480 |
| **5** | GB/T 879 1 | Elastic (Spring) pin ⌀20x60mm | 65Mn | Slotted spring pins | - | 384 |
| **6** | FH1215.8175.AIA.06-10 | Solid dowel pin ⌀22x75mm | GCr15 | Flat vented, pull out dowel pin | - | 192 |
| **7** | GB5783-86 | M30-3.5x80 Bolt | 8.8 Grade | Hex head | Dacro | 288 |
| **8** | GB5783-86 | M30-3.5x85 Bolt | 8.8 Grade | Hex head | Dacro | 240 |
| **9** | GB/T 879 1 | Elastic (Spring) pin ⌀30x70mm | 65Mn | Slotted spring pins | - | 240 |
| **10** | FH1215.8175.AIA.07-17 | Solid dowel pin ⌀32x86mm | GCr15 | Flat vented, pull out dowel pin | - | 240 |
| **11** | Nordlock washer | NL20ss | Stainless Steel | - | - | 288 |
| **12** | Nordlock washer | NL30ss | Stainless Steel | - | - | 288 |
| **13** |  - | Stainless steel wire (2mm dia) | Stainless Steel | - | - | 1 lot |