**East Jordan / Kom. 11188**

Supports :

* 84 parts of hexagon screw M30 x 160 ISO 4014 strength 10.9
* 84 parts of lock washer S30
* 84 parts of hexagon nut M30 ISO 4032 strength 10
* 168 parts of washer Ø31/Ø56x5 DIN EN 14399
* 16 parts of clamping sleeve Ø20 x 60 ISO 8752
* 48 parts of hexagon screw M36 x 150 ISO 4017 strength 10.9
* 16 parts of cylinder screw M36 x 260 ISO 4762 strength 10.9
* 64 parts of lock washer S36
* 64 parts of washer Ø37/Ø66x6 DIN EN 14399
* 6 parts of clamping sleeve Ø20 x 90 ISO 8752

Turntable :

* 16 parts of cylinder screw M36 x 180 ISO 4762 strength 10.9
* 16 parts of lock washer S36
* 16 parts of washer Ø37/Ø66x6 DIN EN 14399
* 16 parts of cylinder screw M30 x 130 ISO 4762 strength 10.9
* 16 parts of lock washer S30

Squeeze head transport (bearing blocks):

* 4 parts of cylinder screw M20 x 90 ISO 4762 strength 8.8
* 8 parts of cylinder screw M20 x 60 ISO 4762 strength 8.8
* 12 parts of lock washer S20

31.10.2018

V. Blöcher