|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **PIPE CLASS** | **PRODUCT** | **(NPS)** | **(NPS)** | **(NPS)** | **FURTHER DETAILS** | **MATERIAL** | **QTY** |  |
| B43 | BOLT | 3/4" | 3/4" |  | 110 STUD BOLT + 2 HEAVY NUTS ASME B1.1 (UNC <= 1" & 8 UN =>1 1/8) ASME 18.2.2/1 HOT DIP GALVANIZED ACC. TO ASTM A 153 | ASTM A 193 Gr.B7M - A 194 Gr.2HM | 24 | pcs |
| B43 | BOLT | 3/4" | 3/4" |  | 105 STUD BOLT + 2 HEAVY NUTS ASME B1.1 (UNC <= 1" & 8 UN =>1 1/8) ASME 18.2.2/1 HOT DIP GALVANIZED ACC. TO ASTM A 153 | ASTM A 193 Gr.B7M - A 194 Gr.2HM | 24 | pcs |
| B43 | BOLT | 5/8" | 5/8" |  | 95 STUD BOLT + 2 HEAVY NUTS ASME B1.1 (UNC <= 1" & 8 UN =>1 1/8) ASME 18.2.2/1 HOT DIP GALVANIZED ACC. TO ASTM A 153 | ASTM A 193 Gr.B7M - A 194 Gr.2HM | 16 | pcs |
| B43 | GASK | 2" | 2" |  | GASKET SPIRAL WOUND THK. 3.2 MM ASME B16.20 300 LB CENTERING & INNER RING | AISI 316 + GRAPHITE | 5 | pcs |
| B43 | GASK | 3" | 3" |  | GASKET SPIRAL WOUND THK. 3.2 MM ASME B16.20 300 LB CENTERING & INNER RING | AISI 316 + GRAPHITE | 5 | pcs |
| B43 | GASK | 6" | 6" |  | GASKET SPIRAL WOUND THK. 3.2 MM ASME B16.20 300 LB CENTERING & INNER RING | AISI 316 + GRAPHITE | 5 | pcs |
| A42 | BOLT | 3/4" | 3/4" |  | 110 STUD BOLT + 2 HEAVY NUTS ASME B1.1 (UNC <= 1" & 8 UN =>1 1/8) ASME 18.2.2/1 HOT DIP GALVANIZED ACC. TO ASTM A 153 | ASTM A 193 Gr.B7M - A 194 Gr.2HM | 16 | pcs |
| A42 | BOLT | 5/8" | 5/8" |  | 105 STUD BOLT + 2 HEAVY NUTS ASME B1.1 (UNC <= 1" & 8 UN =>1 1/8) ASME 18.2.2/1 HOT DIP GALVANIZED ACC. TO ASTM A 153 | ASTM A 193 Gr.B7M - A 194 Gr.2HM | 24 | pcs |
| A42 | BOLT | 5/8" | 5/8" |  | 140 STUD BOLT + 2 HEAVY NUTS ASME B1.1 (UNC <= 1" & 8 UN =>1 1/8) ASME 18.2.2/1 HOT DIP GALVANIZED ACC. TO ASTM A 153 | ASTM A 193 Gr.B7M - A 194 Gr.2HM | 8 | pcs |
| A42 | BOLT | 5/8" | 5/8" |  | 105 STUD BOLT + 2 HEAVY NUTS ASME B1.1 (UNC <= 1" & 8 UN =>1 1/8) ASME 18.2.2/1 HOT DIP GALVANIZED ACC. TO ASTM A 153 | ASTM A 193 Gr.B7M - A 194 Gr.2HM | 8 | pcs |
| A42 | BOLT | 5/8" | 5/8" |  | 95 STUD BOLT + 2 HEAVY NUTS ASME B1.1 (UNC <= 1" & 8 UN =>1 1/8) ASME 18.2.2/1 HOT DIP GALVANIZED ACC. TO ASTM A 153 | ASTM A 193 Gr.B7M - A 194 Gr.2HM | 8 | pcs |
| A42 | GASK | 3" | 3" |  | GASKET SPIRAL WOUND THK. 3.2 MM ASME B16.20 150 LB CENTERING & INNER RING | AISI 316 + GRAPHITE | 5 | pcs |
| A42 | GASK | 3/4" | 3/4" |  | GASKET SPIRAL WOUND THK. 3.2 MM ASME B16.20 600 LB CENTERING & INNER RING | AISI 316 + GRAPHITE | 5 | pcs |
| A42 | GASK | 4" | 4" |  | GASKET SPIRAL WOUND THK. 3.2 MM ASME B16.20 150 LB CENTERING & INNER RING | AISI 316 + GRAPHITE | 5 | pcs |
| A42 | GASK | 6" | 6" |  | GASKET SPIRAL WOUND THK. 3.2 MM ASME B16.20 150 LB CENTERING & INNER RING | AISI 316 + GRAPHITE | 5 | pcs |