INQUIRY NUM. DH-21-016

ITEM QTY UNIT DESCRIPTION

9 100 SET HEX HEAD CAP SCREW 5/8” X 2-1/2” FULL

THREADED. MATERIAL SA 1018.

ASTM A 307 GRADE B CARBON STEEL WITH -

HEXAGONAL NUT ASTM A-563 GRADE B.

10 350 SET HEX HEAD CAP SCREW ½” X 1-1/2”

ASTM A 307 GRADE B CARBON STEEL WITH -

HEXAGONAL NUT SAE-J995 GRADE 5.

11 350 PC ROUND PLAIN WASHER ½” DIAM FORGED CARBON STEEL.

54 100 SET HEX HEAD CAP SCREW STD THREAD 3/8” X

2-1/2” ASTM A-307 GRADE A CARBON STEEL WITH HEXAGONAL NUT A-194 2H.

55 100 PC STANDARD LOCK WASHER ASTM F 436 FOR

3/8” DIA BOLT .

56 100 SET HEX HEAD CAP SCREW STD THREAD ½” X

2-1/2” ASTM A 307 GRADE B CARBON STEEL

WITH HEXAGONAL NUT SAE-J995 GRADE 5.

57 100 PC LOCK WASHER 1/2” DIAM. CARBON STEEL.

59 20 SET “U” BOLT ½” DIAM. FOR 3” DIAM PIPE, GALVA- NIZED, WITH HEXAGONAL NUTS AND LOCK WA-

½” DIAM.

60 10 SET “U” BOLT ½” DIAM FOR PIPE 4” DIAM , GALVA-

NIZED WITH HEXAGONAL NUTS AND LOCK WA-

SHERS.