

November 5, 2021

Re: Our RFQ # 460933

Please quote your best price and delivery, resale discount, shipping point, and estimated packaged size/weight for determination of freight costs.

Note 1: All studs need to include 2 nuts & 2 washers per stud.

Note 2: Material - Stainless steel B8M class 2 – AISI 316SS, Carbide Solution Treated, Strain Hardened

**QTY** **SIZE**

80 ½" x 3"

732 ⅝" x 3½"

140 ⅝" x 4"

68 ⅝" x 6½"

48 ¾" x 4"

80 ¾" x 5"

36 ¾" x 7"

36 ¾" x 8"

110 ⅞" x 6½"

72 ⅞" x 8½"

If any of these lengths do not meet your standard production sizes, please include an optional quote on the next longest length that does meet standard production.

Contact Mike Wolford at 985-888-1900 or 504-915-7703 (Cell), or via email at mike@morlandsupply.com

with any questions.