|  |  |  |
| --- | --- | --- |
| **Material** | **Description** | **Qty.** |
| GALVANIZED | LOCK WASHER Ø8 | 8 |
| STAINLESS STEEL. 316 | FLAT WASHER MEDIANA Ø1/2" | 2 |
| STAINLESS STEEL 304 | FLAT WASHER MEDIANA Ø3/8" | 2 |
| STAINLESS STEEL 304 | FLAT WASHER MEDIANA Ø3/8" | 12 |
| F-436 ZINC. | FLAT WASHER Ø1/2" | 4 |
| F-436 ZINC. | FLAT WASHER Ø1/2" | 4 |
| F-436 ZINC. | FLAT WASHER Ø1/2" | 4 |
| F-436 GALVANIZED | FLAT WASHER Ø3/8" | 4 |
| F-436 ZINC. | FLAT WASHER Ø5/8" | 4 |
| ASTM A193 GR B8ML | HEX. BOLT  1/2" - 13 UNC x 1 3/4"  | 2 |
| ASTM A193 GR B8 | HEX. BOLT  3/8" - 16 UNC x 1 1/4" | 12 |
| ASTM A193 GR B8M | HEX. BOLT  3/8" - 16 UNC x 2 3/4"  | 2 |
| GR. 2 ZINC. | HEX. BOLT 1/2" - 13 UNC x 2"  | 4 |
| GR. 2 ZINC. | HEX. BOLT 1/2" - 13 UNC x 2"  | 4 |
| GR. 2 GALVANIZED | HEX. BOLT 1/2" - 13 UNC x 4 1/2"  | 4 |
| GR. 2 GALVANIZED | HEX. BOLT 5/8" - 11 UNC x 5"  | 4 |
| GR. 5 GALVANIZED | HEX. BOLT Ø3/8" - 16 UNC x 1 1/2"  | 4 |
| ASTM A194 GR 8M | HEX. NUT  1/2" - 13 UNC | 4 |
| ASTM A194 GR 8 | HEX. NUT  3/8" - 16 UNC | 4 |
| ASTM A194 GR 8 | HEX. NUT  3/8" - 16 UNC | 12 |
| GR. 5 GALVANIZED | HEX. NUT 3/8" -16 UNC | 4 |
| GR. 2 ZINC. | HEX. NUT 5/8" - 11 UNC | 4 |
| GR. 2 ZINC. | HEX. NUT Ø1/2" - 13 UNC | 4 |
| GR. 2 ZINC. | HEX. NUT Ø1/2" - 13 UNC | 4 |
| GR. 2 ZINC. | HEX. NUT Ø1/2" - 13 UNC | 4 |
| CL.8.8 GALVANIZED | BOLT HEX. M8 (5/16) X 20 RC | 8 |