|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| Part No |  | qty |  |  | Description |  | Quantity |
| 80-077090 |  544 |   | Heavy hex. Locknut 1"-8UNC-2B, A194-2H, zinc plated | 544 |
| 80-086328 |  1424 |   | Heavy hex. Locknut 5/8"-11UNC-2B, A194-2H, zinc plated, nylon insert | 1424 |
| 80-091463 | 40  |   | Heavy hex. locknut 3/4"-10UNC-2B, A194-2H, zinc plated, nylon insert | 40 |
| 80-086090 | 852  |   | Heavy hex. Locknut 1 1/8"-8UN-2B, A194-2H, zinc plated, no nylon insert, ASME B18.16.6 Table 3 | 852 |
| 80-085190  | 100  |   | Heavy hex. locknut 1 1/8"-8UN-2B A-194 Gr.2H Stamp Marking ASME II-A Zinc Plated, nylon insert | 100 |
| 80-091462 | 100  |   | Heavy hex. locknut 1"-8UNC-2B A-194 Gr.2H Stamp marking ASME II-A Zinc Plated, nylon insert | 100 |
| 80-090981 | 100  |   | Heavy hex. locknut 1 3/4"-8 UN-2B A-194 Gr.2H Stamp Marking ASME II-A Zinc Plated, nylon insert | 100 |
| 80-082702 | 200  |   | Heavy hex. locknut M24 acc. to ISO 7040 or equivalent A-194 Gr.2H Stamp Marking ASME II-A Zinc Plated, nylon insert | 200 |
| 80-089927 | 100  |   | Heavy hex. locknut 1 3/8"-8UN-2B A-194 Gr.2H Stamp Marking ASME II-A Zinc Plated, NYLON INSERT | 100 |