|  |
| --- |
| **Can I get A price quota on all the screws listed and price breakdown for ordering 1000 screw for each part number listed. All screws are in Metric.**  |
| part number   **L22258-50-6CCR**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw CC = cres Z10 CNT 18-11    Ts Min= 540 MPa (recommended material) Diameter 5mm length 6 sand blasted head painted dull black for cockpit screws (R) (screws in cock pit ) |
|  |
| part number   **L22258-50-6CC**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw CC = cres Z10 CNT 18-11    Ts Min= 540 MPa (recommended material) Diameter 5mm length 6  |
| part number   **L22258-50-6BCLT**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw BC = 35 NC6 steel Ts min = 880 MPa (recommended material)Diameter 5mm length 6 black cadmium plating :LT (screws in cock pit ) |
|  |
| part number   **L22258-50-6BC**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw BC = 35 NC6 steel Ts min = 880 MPa (recommended material)Diameter 5mm length 6  |
| part number   **L22258-50-6BE**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw BE = L or M –LE or ME cadmium plating (recommended material) Diameter 5mm length 6  |
|  |
| part number   **22258TK050006XA**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw TK = T-A6V Titanium TS min= 880 MPa (recommended material) XA= against fretting corrosionDiameter 5mm length 6  |
|  |
| part number   **L22258-50-6CF**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw CF= CRES Z 15 CN 17-03 TS min = 880 MPa (recommended material)Diameter 5mm length 6  |
|  |
| part number   **L22258-50-10TKXA**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw TK = T-A6V Titanium TS min= 880 MPa (recommended material) XA= against fretting corrosionDiameter 5mm length 10  |
| part number   **L22258-50-10CC**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw CC = CRES Z10 CNT 18-11      TS Min= 540 MPa (recommended material) Diameter 5mm length 10 |
|  |
| part number   **L22258-50-10BC**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw BC = 35 NC6 steel TS min = 880 MPa (recommended material)Diameter 5mm length 10  |
| part number   **22258BC050005L**breakdown of part  (Philips head )100 degree csk head , short thread Precision Screw BC = 35 NC6 steel TS min = 880 MPa (recommended material)Diameter 5mm length 5  |
|  |
| part number   **22208BE050012L** |
| part number   **22208BC040010LT** |
| part number  (bolt)  **F161-10816** |
| part number  (nut)  **22453bc050LE** |